Here you see the heatsink is made of aluminum with a thin rubber insulation pad:
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Here i have cut away an area around the battery lead soldering points and i have removed the paper label underneath the heat sink, and applied silver-paste before placing the heat sink (wich came from an old PC video card) and used 2 small cable binder to keep the heatsink in place
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here you seeen there is no more gap between the mosfets and the heat sink
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And finished the edges with electrical tape. It does not look pretty but it is functional and no more risk of shorting out the esc .

[image: image4.jpg]



Of course if yout want to do this with your own esc, it is on you own risk. It's stilll hobby-ing around. 
